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IDEAL LUX · ARCHIMEDE COLLECTION · PENDANTS · INDOOR
Archimede SP Cono Black
Powder coated metal ceiling cap with magnetic closure without screws. PVC cable. Powder coated aluminum diffuser with acrylic optic. Finishes: white, black.
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Specification
	Dimensions
	Ø 90 × H min 375 / max 6150 mm

	Light source
	LED 4W

	LED lifetime
	50000 hours

	Colour temperature
	3000 K

	Light output (LED source)
	250 lumen

	IP rating
	IP20 (indoor)

	Bulb included
	Integrated LED

	Colour rendering (CRI)
	> 90

	Light output (from fitting)
	210 lm

	Beam angle
	24°

	Dimming
	Non-dimmable, On-Off

	Insulation class
	II

	Operating temperature
	0° ~ +40 °C

	Warranty
	5 years

	Net weight
	0.14 kg

	EAN
	8021696328348

	Product code
	328348



UK retail price: £70.00 ex VAT  ·  £84.00 inc VAT
Trade, project and quantity pricing on request. Delivery and lead time confirmed at order.
Specification from the Ideal Lux technical sheet rev. 22-07-2026, checked 2026-10-02. Manufacturer data may change; confirm before ordering. Images © Ideal Lux.
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