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IDEAL LUX · ARGO COLLECTION · OUTDOOR LIGHTING
Argo AP1 3000K
Powder coated die-cast aluminum body. Clear tempered glass diffuser with white inner reflector. Available in anthracite or white finish.
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Specification
	Dimensions
	L 90 × H 102 × D 55 mm  (L length, H height, D depth)

	Light source
	Integrated LED 6W

	LED lifetime
	30000 hours

	Colour temperature
	3000 K

	Light output (LED source)
	550 lumen

	IP rating
	IP65 (outdoor rated)

	Bulb included
	Integrated LED

	Colour rendering (CRI)
	> 90

	Light output (from fitting)
	400 lm

	Beam angle
	100°

	Dimming
	Non-dimmable, On-Off

	Insulation class
	I

	Operating temperature
	-15° ~ +45 °C

	Warranty
	5 years

	Net weight
	0.6 kg

	EAN
	8021696321646

	Product code
	321646



UK retail price: £71.00 ex VAT  ·  £85.20 inc VAT
Trade, project and quantity pricing on request. Delivery and lead time confirmed at order.
Specification from the Ideal Lux technical sheet rev. 21-07-2026, checked 2026-10-02. Manufacturer data may change; confirm before ordering. Images © Ideal Lux.
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