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	SPECIFICATION SHEET
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IDEAL LUX · LITE COLLECTION · WALL LIGHTS · INDOOR
Lite AP
Aluminium base and body with white, black, nickel or brass finish. Adjustable diffuser. Integrated switch. Recessed installation on flush-mounting box type 502, not included.
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Specification
	Dimensions
	L 85 × H 85 × D 90 mm  (L length, H height, D depth)

	Light source
	LED 3W

	LED lifetime
	20000 hours

	Colour temperature
	3000 K

	Light output (LED source)
	200 lumen

	IP rating
	IP20 (indoor)

	Bulb included
	Integrated LED

	Colour rendering (CRI)
	> 90

	Light output (from fitting)
	180 lm

	Beam angle
	23°

	Dimming
	1, Touch dimmer

	Insulation class
	I

	Operating temperature
	0° ~ +40 °C

	Warranty
	5 years

	Net weight
	0.34 kg

	EAN
	8021696250106

	Product code
	250106



UK retail price: £69.00 ex VAT  ·  £82.80 inc VAT
Trade, project and quantity pricing on request. Delivery and lead time confirmed at order.
Specification from the Ideal Lux technical sheet rev. 21-07-2026, checked 2026-10-01. Manufacturer data may change; confirm before ordering. Images © Ideal Lux.
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